# Firmware Update

This lets you install a new version of the Pinscape firmware onto your KL25Z, preserving your current configuration settings.

Pinscape Unit | KL25Z CPU ID | OpenSDA ID
Currently installed firmware build:

## Step 1: Select a firmware version to install

Pinscape Downloads:
(No firmware versions have been downloaded)
Browse for a file
File selected:

## Step 2: Save current settings

Before proceeding, we'll save the current configuration settings on this KL25Z so that they can be restored after the firmware update.
Please make sure the KL25Z is plugged in via the joystick port, as shown at right. This will allow reading the current configuration settings for backup.
Saving settings to disk...
Saved to

## Step 3: Plug in programming port

We're ready to install the new firmware. Please make sure the programming port on the KL25Z is plugged in, as shown in the diagram at right. If everything's okay, the small green LED next to the programming port should be on (not flashing). If the green LED is flashing, try unplugging all cables from the device for a few seconds, then plug the programming port back in.
It's fine to leave both ports plugged in throughout the update. But if you only have one cable, simply unplug the joystick port now and move the cable over to the programming port.
The software should detect the drive when you plug it in and automatically advance to the next step. If these instructions are still showing, the software hasn't detected the port yet. Select the drive manually
Warning: it looks like more than one KL25Z programming port is plugged in. If you know which one is which, you can click on it in the list above - but if there's any doubt, the easiest way to clear it up is to make sure that the only one plugged in is the one you want to program.
Programming drive: ()

## Step 4: Install firmware

We're ready to go! Install now
Firmware updated!

## Step 5: Plug in joystick port

The new firmware has been installed, so we're ready to restore your configuration settings. Please make sure the KL25Z is plugged in via the joystick port, as shown at right.
If you moved your USB cable over to the programming port for the previous step, you can now unplug it and move it back to the joystick port. It's also okay to leave both ports plugged in.
Done

## Step 6: Restore settings

Restoring settings from ...
Settings restored

## Done!

The firmware update was successfully completed.