# Main Menu

Welcome! This program helps you set up and configure your Pinscape Controller units.
An updated version of this program is available - Install Now

(Searching for devices...)

To connect a controller that you've already set up, plug a USB cable into the joystick port on the KL25Z as shown at right, and plug the other end into a free USB port on your PC.
(The other USB connector on the KL25Z is the programming port, which is used for installing and updating the firmware. It's fine to leave both ports plugged in, but if you only have one cable, connect it to the joystick port during normal use.)

Set up a new KL25Z
If you have a new KL25Z, this will lead you through the steps to prepare it for use and install the Pinscape firmware.

Software updates Enable auto download View downloads folder More...
The setup tool can automatically check for and download updates each time you run it. If this feature is enabled, updates to the setup tool and firmware will be downloaded automatically. You'll be notified when new updates are ready to install.
Download status: Initializing Check again | Check manually
Config tool: Update available - Install Now
Config tool: Up to date
Firmware: Checking

Miscellaneous
Restore hidden dialogs [?]
Some warning dialogs offer a checkbox saying "Don't show me this message again", in case you're tired of seeing the same advice over and over. This button un-checks all of those checkboxes so that the dialogs will appear again when appropriate.
Important DOF & LEDWIZ.DLL updates

About this project More...
This is build of the Config Tool.
The Pinscape Controller is a free, open-source software and hardware project. You can find the source code, documentation, and more on our mbed.org project page.
Loading...